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sion housing and allow the oil to run out.
Check that the plug O-ring is fault free; replace as
necessary.

Install the plug and O-ring.

Fill with oil to the correct level through the oil dip-
stick hole. For oil grade and quantity, refer to the
Technical Data page 71 section.

Itis also possible to replace oil without laying up the
boat, e.g. if the oil change interval is reached during
the season. Pump out the oil through a suction pipe
using an oil drain pump — this method leaves approx.
0.5 liter (0.15 US gbl) remaining in the stern drive. Fill
with oil to the correct level through the oil dipstick hole.
For oil grade, refer to the Technical Data page 71
section.

The oil should have a golden brown nuance. If the oil
is gray, water has entered the stern drive. In this case
let a Volvo Penta workshop carry out checks on the
stern drive.





